**[MS-OXRTFCP]:**

**Rich Text Format (RTF) Compression Algorithm**

Intellectual Property Rights Notice for Open Specifications Documentation

* **Technical Documentation.** Microsoft publishes Open Specifications documentation (“this documentation”) for protocols, file formats, data portability, computer languages, and standards support. Additionally, overview documents cover inter-protocol relationships and interactions.
* **Copyrights**. This documentation is covered by Microsoft copyrights. Regardless of any other terms that are contained in the terms of use for the Microsoft website that hosts this documentation, you can make copies of it in order to develop implementations of the technologies that are described in this documentation and can distribute portions of it in your implementations that use these technologies or in your documentation as necessary to properly document the implementation. You can also distribute in your implementation, with or without modification, any schemas, IDLs, or code samples that are included in the documentation. This permission also applies to any documents that are referenced in the Open Specifications documentation.
* **No Trade Secrets**. Microsoft does not claim any trade secret rights in this documentation.
* **Patents**. Microsoft has patents that might cover your implementations of the technologies described in the Open Specifications documentation. Neither this notice nor Microsoft's delivery of this documentation grants any licenses under those patents or any other Microsoft patents. However, a given Open Specifications document might be covered by the Microsoft [Open Specifications Promise](https://go.microsoft.com/fwlink/?LinkId=214445) or the [Microsoft Community Promise](https://go.microsoft.com/fwlink/?LinkId=214448). If you would prefer a written license, or if the technologies described in this documentation are not covered by the Open Specifications Promise or Community Promise, as applicable, patent licenses are available by contacting iplg@microsoft.com.
* **License Programs**. To see all of the protocols in scope under a specific license program and the associated patents, visit the [Patent Map](https://aka.ms/AA9ufj8).
* **Trademarks**. The names of companies and products contained in this documentation might be covered by trademarks or similar intellectual property rights. This notice does not grant any licenses under those rights. For a list of Microsoft trademarks, visit [www.microsoft.com/trademarks](https://www.microsoft.com/trademarks).
* **Fictitious Names**. The example companies, organizations, products, domain names, email addresses, logos, people, places, and events that are depicted in this documentation are fictitious. No association with any real company, organization, product, domain name, email address, logo, person, place, or event is intended or should be inferred.

**Reservation of Rights**. All other rights are reserved, and this notice does not grant any rights other than as specifically described above, whether by implication, estoppel, or otherwise.

**Tools**. The Open Specifications documentation does not require the use of Microsoft programming tools or programming environments in order for you to develop an implementation. If you have access to Microsoft programming tools and environments, you are free to take advantage of them. Certain Open Specifications documents are intended for use in conjunction with publicly available standards specifications and network programming art and, as such, assume that the reader either is familiar with the aforementioned material or has immediate access to it.

**Support.** For questions and support, please contact dochelp@microsoft.com.

**Preliminary Documentation.** This particular Open Specifications document provides documentation for past and current releases and/or for the pre-release version of this technology. This document provides final documentation for past and current releases and preliminary documentation, as applicable and specifically noted in this document, for the pre-release version. Microsoft will release final documentation in connection with the commercial release of the updated or new version of this technology. Because this documentation might change between the pre-release version and the final version of this technology, there are risks in relying on this preliminary documentation. To the extent that you incur additional development obligations or any other costs as a result of relying on this preliminary documentation, you do so at your own risk.

**Revision Summary**

| Date | Revision History | Revision Class | Comments |
| --- | --- | --- | --- |
| 4/4/2008 | 0.1 | New | Initial Availability. |
| 4/25/2008 | 0.2 | Minor | Revised and updated property names and other technical content. |
| 6/27/2008 | 1.0 | Major | Initial Release. |
| 8/6/2008 | 1.01 | Minor | Updated references to reflect date of initial release. |
| 9/3/2008 | 1.02 | Minor | Revised and edited technical content. |
| 12/3/2008 | 1.03 | Minor | Updated IP notice. |
| 3/4/2009 | 1.04 | Minor | Revised and edited technical content. |
| 4/10/2009 | 2.0 | Major | Updated applicable product releases. |
| 7/15/2009 | 3.0 | Major | Revised and edited for technical content. |
| 11/4/2009 | 3.1 | Minor | Updated the technical content. |
| 2/10/2010 | 3.2 | Minor | Updated the technical content. |
| 5/5/2010 | 3.3 | Minor | Updated the technical content. |
| 8/4/2010 | 3.4 | Minor | Clarified the meaning of the technical content. |
| 11/3/2010 | 3.4 | None | No changes to the meaning, language, or formatting of the technical content. |
| 3/18/2011 | 3.4 | None | No changes to the meaning, language, or formatting of the technical content. |
| 8/5/2011 | 4.0 | Major | Significantly changed the technical content. |
| 10/7/2011 | 4.0 | None | No changes to the meaning, language, or formatting of the technical content. |
| 1/20/2012 | 5.0 | Major | Significantly changed the technical content. |
| 4/27/2012 | 6.0 | Major | Significantly changed the technical content. |
| 7/16/2012 | 7.0 | Major | Significantly changed the technical content. |
| 10/8/2012 | 7.1 | Minor | Clarified the meaning of the technical content. |
| 2/11/2013 | 7.2 | Minor | Clarified the meaning of the technical content. |
| 7/26/2013 | 7.2 | None | No changes to the meaning, language, or formatting of the technical content. |
| 11/18/2013 | 7.2 | None | No changes to the meaning, language, or formatting of the technical content. |
| 2/10/2014 | 7.2 | None | No changes to the meaning, language, or formatting of the technical content. |
| 4/30/2014 | 7.2 | None | No changes to the meaning, language, or formatting of the technical content. |
| 7/31/2014 | 7.2 | None | No changes to the meaning, language, or formatting of the technical content. |
| 10/30/2014 | 7.2 | None | No changes to the meaning, language, or formatting of the technical content. |
| 3/16/2015 | 8.0 | Major | Significantly changed the technical content. |
| 5/26/2015 | 8.1 | Minor | Clarified the meaning of the technical content. |
| 9/14/2015 | 8.1 | None | No changes to the meaning, language, or formatting of the technical content. |
| 6/13/2016 | 9.0 | Major | Significantly changed the technical content. |
| 9/14/2016 | 9.0 | None | No changes to the meaning, language, or formatting of the technical content. |
| 7/24/2018 | 10.0 | Major | Significantly changed the technical content. |
| 10/1/2018 | 11.0 | Major | Significantly changed the technical content. |
| 4/22/2021 | 12.0 | Major | Significantly changed the technical content. |

Table of Contents

[1 Introduction 7](#_Toc69362031)

[1.1 Glossary 7](#_Toc69362032)

[1.2 References 7](#_Toc69362033)

[1.2.1 Normative References 8](#_Toc69362034)

[1.2.2 Informative References 8](#_Toc69362035)

[1.3 Overview 8](#_Toc69362036)

[1.4 Relationship to Protocols and Other Algorithms 8](#_Toc69362037)

[1.5 Applicability Statement 8](#_Toc69362038)

[1.6 Standards Assignments 8](#_Toc69362039)

[2 Algorithm Details 9](#_Toc69362040)

[2.1 Common Algorithm Details 9](#_Toc69362041)

[2.1.1 Abstract Data Model 9](#_Toc69362042)

[2.1.2 Initialization 9](#_Toc69362043)

[2.1.2.1 Dictionary 9](#_Toc69362044)

[2.1.2.2 CRC 9](#_Toc69362045)

[2.1.2.2.1 CRC Lookup Table 9](#_Toc69362046)

[2.1.3 Processing Rules 11](#_Toc69362047)

[2.1.3.1 RTF Compression Format 11](#_Toc69362048)

[2.1.3.1.1 RTF Compression ABNF Grammar 11](#_Toc69362049)

[2.1.3.1.2 Compressed RTF 11](#_Toc69362050)

[2.1.3.1.3 Compressed Run 12](#_Toc69362051)

[2.1.3.1.4 Dictionary 12](#_Toc69362052)

[2.1.3.1.5 Dictionary Reference 12](#_Toc69362053)

[2.1.3.2 Calculate a CRC from a Given Array of Bytes 13](#_Toc69362054)

[2.2 Decompression Algorithm Details 13](#_Toc69362055)

[2.2.1 Abstract Data Model 13](#_Toc69362056)

[2.2.1.1 Input and Output 13](#_Toc69362057)

[2.2.2 Initialization 13](#_Toc69362058)

[2.2.2.1 Header 14](#_Toc69362059)

[2.2.2.2 Output 14](#_Toc69362060)

[2.2.3 Processing Rules 14](#_Toc69362061)

[2.2.3.1 Decompressing Input of COMPTYPE UNCOMPRESSED 14](#_Toc69362062)

[2.2.3.2 Decompressing Input of COMPTYPE COMPRESSED 14](#_Toc69362063)

[2.3 Compression Algorithm Details 15](#_Toc69362064)

[2.3.1 Abstract Data Model 15](#_Toc69362065)

[2.3.1.1 Input and Output 15](#_Toc69362066)

[2.3.1.2 Run Information 15](#_Toc69362067)

[2.3.2 Initialization 16](#_Toc69362068)

[2.3.2.1 Input and Output 16](#_Toc69362069)

[2.3.3 Processing Rules 16](#_Toc69362070)

[2.3.3.1 Compressing a Buffer of Uncompressed Contents with COMPTYPE UNCOMPRESSED 16](#_Toc69362071)

[2.3.3.1.1 Filling in the Header 16](#_Toc69362072)

[2.3.3.2 Compressing a Buffer of Uncompressed Contents with COMPTYPE COMPRESSED 16](#_Toc69362073)

[2.3.3.2.1 Finding the Longest Match to Input 17](#_Toc69362074)

[2.3.3.2.2 Filling in the Header 19](#_Toc69362075)

[3 Algorithm Examples 20](#_Toc69362076)

[3.1 Decompressing Compressed RTF 20](#_Toc69362077)

[3.1.1 Example 1: Simple Compressed RTF 20](#_Toc69362078)

[3.1.1.1 Compressed RTF Data 20](#_Toc69362079)

[3.1.1.2 Compressed RTF Header 20](#_Toc69362080)

[3.1.1.3 Initialization 20](#_Toc69362081)

[3.1.1.4 Run 1 20](#_Toc69362082)

[3.1.1.5 Run 2 23](#_Toc69362083)

[3.1.1.6 Run 3 24](#_Toc69362084)

[3.1.2 Example 2: Reading a Token from the Dictionary that Crosses WritePosition 25](#_Toc69362085)

[3.1.2.1 Compressed RTF 25](#_Toc69362086)

[3.1.2.2 Compressed RTF Header 25](#_Toc69362087)

[3.1.2.3 Initialization 25](#_Toc69362088)

[3.1.2.4 Run 1 25](#_Toc69362089)

[3.1.2.5 Run 2 27](#_Toc69362090)

[3.2 Generating Compressed RTF 28](#_Toc69362091)

[3.2.1 Example 1: Simple RTF 28](#_Toc69362092)

[3.2.1.1 Initialization 28](#_Toc69362093)

[3.2.1.2 Run 1 29](#_Toc69362094)

[3.2.1.3 Run 2 33](#_Toc69362095)

[3.2.1.4 Run 3 35](#_Toc69362096)

[3.2.2 Example 2: Compressing with Tokens that Cross WritePosition 37](#_Toc69362097)

[3.2.2.1 Initialization 37](#_Toc69362098)

[3.2.2.2 Run 1 38](#_Toc69362099)

[3.2.2.3 Run 2 40](#_Toc69362100)

[3.3 Generating the CRC 41](#_Toc69362101)

[3.3.1 Example of CRC Generation 41](#_Toc69362102)

[3.3.1.1 Initialization 41](#_Toc69362103)

[3.3.1.2 First Byte 41](#_Toc69362104)

[3.3.1.3 Second Byte 42](#_Toc69362105)

[3.3.1.4 Continuation 42](#_Toc69362106)

[4 Security 43](#_Toc69362107)

[4.1 Security Considerations for Implementers 43](#_Toc69362108)

[4.2 Index of Security Parameters 43](#_Toc69362109)

[5 Appendix A: Product Behavior 44](#_Toc69362110)

[6 Change Tracking 45](#_Toc69362111)

[7 Index 46](#_Toc69362112)

# Introduction

The Rich Text Format (RTF) Compression Algorithm is used to compress and decompress [**RTF**](#gt_a9aa8673-7798-4eba-a048-8b7c95a7b080) data, as described in [[MSFT-RTF]](https://go.microsoft.com/fwlink/?LinkId=120924), to or from one of the supported compression formats.

Sections 1.6 and 2 of this specification are normative. All other sections and examples in this specification are informative.

## Glossary

This document uses the following terms:

**ASCII**: The American Standard Code for Information Interchange (ASCII) is an 8-bit character-encoding scheme based on the English alphabet. ASCII codes represent text in computers, communications equipment, and other devices that work with text. ASCII refers to a single 8-bit ASCII character or an array of 8-bit ASCII characters with the high bit of each character set to zero.

**Augmented Backus-Naur Form (ABNF)**: A modified version of Backus-Naur Form (BNF), commonly used by Internet specifications. ABNF notation balances compactness and simplicity with reasonable representational power. ABNF differs from standard BNF in its definitions and uses of naming rules, repetition, alternatives, order-independence, and value ranges. For more information, see [[RFC5234]](https://go.microsoft.com/fwlink/?LinkId=123096).

**big-endian**: Multiple-byte values that are byte-ordered with the most significant byte stored in the memory location with the lowest address.

**cyclic redundancy check (CRC)**: An algorithm used to produce a checksum (a small, fixed number of bits) against a block of data, such as a packet of network traffic or a block of a computer file. The CRC is a broad class of functions used to detect errors after transmission or storage. A CRC is designed to catch random errors, as opposed to intentional errors. If errors might be introduced by a motivated and intelligent adversary, a cryptographic hash function should be used instead.

**little-endian**: Multiple-byte values that are byte-ordered with the least significant byte stored in the memory location with the lowest address.

**Message object**: A set of properties that represents an email message, appointment, contact, or other type of personal-information-management object. In addition to its own properties, a Message object contains recipient properties that represent the addressees to which it is addressed, and an attachments table that represents any files and other Message objects that are attached to it.

**Rich Text Format (RTF)**: Text with formatting as described in [[MSFT-RTF]](https://go.microsoft.com/fwlink/?LinkId=120924).

**MAY, SHOULD, MUST, SHOULD NOT, MUST NOT:** These terms (in all caps) are used as defined in [[RFC2119]](https://go.microsoft.com/fwlink/?LinkId=90317). All statements of optional behavior use either MAY, SHOULD, or SHOULD NOT.

## References

Links to a document in the Microsoft Open Specifications library point to the correct section in the most recently published version of the referenced document. However, because individual documents in the library are not updated at the same time, the section numbers in the documents may not match. You can confirm the correct section numbering by checking the [Errata](https://go.microsoft.com/fwlink/?linkid=850906).

### Normative References

We conduct frequent surveys of the normative references to assure their continued availability. If you have any issue with finding a normative reference, please contact dochelp@microsoft.com. We will assist you in finding the relevant information.

[MS-DTYP] Microsoft Corporation, "[Windows Data Types](%5BMS-DTYP%5D.pdf#Section_cca2742956894a16b2b49325d93e4ba2)".

[MS-OXPROPS] Microsoft Corporation, "[Exchange Server Protocols Master Property List](%5BMS-OXPROPS%5D.pdf#Section_f6ab1613aefe447da49c18217230b148)".

[RFC2119] Bradner, S., "Key words for use in RFCs to Indicate Requirement Levels", BCP 14, RFC 2119, March 1997, [http://www.rfc-editor.org/rfc/rfc2119.txt](https://go.microsoft.com/fwlink/?LinkId=90317)

[RFC5234] Crocker, D., Ed., and Overell, P., "Augmented BNF for Syntax Specifications: ABNF", STD 68, RFC 5234, January 2008, [http://www.rfc-editor.org/rfc/rfc5234.txt](https://go.microsoft.com/fwlink/?LinkId=123096)

### Informative References

[MS-OXPROTO] Microsoft Corporation, "[Exchange Server Protocols System Overview](%5BMS-OXPROTO%5D.pdf#Section_734ab967e43e425babe1974af56c0283)".

[MSFT-RTF] Microsoft Corporation, "Rich Text Format (RTF) Specification", version 1.9.1, March 2008, [https://interoperability.blob.core.windows.net/files/Archive\_References/[MSFT-RTF].pdf](https://go.microsoft.com/fwlink/?LinkId=120924)

## Overview

This algorithm enables an implementer to compress or decompress [**RTF**](#gt_a9aa8673-7798-4eba-a048-8b7c95a7b080)-encoded text. During compression, the RTF-encoded text is compared to a dictionary of RTF control words, as described in [[MSFT-RTF]](https://go.microsoft.com/fwlink/?LinkId=120924). If any of the input text matches the control words in the dictionary, a dictionary reference, as described in section [2.1.3.1.5](#Section_b12474dfe0ef47319315454a49a984d8), is written to the output buffer in place of the control word to reduce the bytes sent over the wire. Any content that does not have a dictionary match is simply written to the output buffer.

Conversely, during decompression, the compressed RTF-encoded text is compared against the dictionary and dictionary references are replaced with RTF control words. This algorithm defines the manner in which the RTF-encoded text is compared to the dictionary content and how the RTF-encoded text is read from the input buffer or written to the output buffer.

## Relationship to Protocols and Other Algorithms

The [**RTF**](#gt_a9aa8673-7798-4eba-a048-8b7c95a7b080) text encoding format is described in [[MSFT-RTF]](https://go.microsoft.com/fwlink/?LinkId=120924). This algorithm requires no additional protocols or algorithms to accomplish the compression format described in this specification. The **PidTagRtfCompressed** property ([[MS-OXPROPS]](%5BMS-OXPROPS%5D.pdf#Section_f6ab1613aefe447da49c18217230b148) section 2.941) relies on this algorithm.

For conceptual background information and overviews of the relationships and interactions between this and other protocols, see [[MS-OXPROTO]](%5BMS-OXPROTO%5D.pdf#Section_734ab967e43e425babe1974af56c0283).

## Applicability Statement

This algorithm is specifically used with information from the **PidTagRtfCompressed** property ([[MS-OXPROPS]](%5BMS-OXPROPS%5D.pdf#Section_f6ab1613aefe447da49c18217230b148) section 2.941) of the [**Message object**](#gt_b6c15d0c-d992-421d-ba96-99d3b63894cf). Clients that do not implement this algorithm are unable to interpret the data that is packed with this algorithm. This algorithm can be used to compress and decompress any content (not just [**RTF**](#gt_a9aa8673-7798-4eba-a048-8b7c95a7b080)). In addition, this algorithm supports the storing of content in an uncompressed form.

## Standards Assignments

None.

# Algorithm Details

## Common Algorithm Details

### Abstract Data Model

This section describes a conceptual model of possible data organization that an implementation maintains to participate in this algorithm. The described organization is provided to facilitate the explanation of how the algorithm behaves. This document does not mandate that implementations adhere to this model as long as their external behavior is consistent with that described in this document.

The following elements are specific to this algorithm:

* **Writer:** Software that writes compressed [**RTF**](#gt_a9aa8673-7798-4eba-a048-8b7c95a7b080) data.
* **Reader:** Software that is capable of reading compressed RTF data and decompressing it into RTF encrypted text.
* **Dictionary:** A 4096-byte circular array of RTF control words. References to the dictionary are used to compress or decompress RTF data.
* **CRC Lookup Table:** A pre-computed table used for **CRC** field generation, as specified in section [2.1.2.2.1](#Section_2500f63ea1ec4605a80dd41ab63e80e9).

### Initialization

#### Dictionary

The writer MUST initialize the dictionary (starting at offset 0) with the following [**ASCII**](#gt_79fa85ca-ac61-467c-b819-e97dc1a7a599) string:

1. {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil<SP>\froman<SP>\fswiss<SP>\fmodern<SP>\fscript<SP>\fdecor<SP>MS<SP>Sans<SP>SerifSymbolArialTimes<SP>New<SP>RomanCourier{\colortbl\red0\green0\blue0<CR><LF>\par<SP>\pard\plain\f0\fs20\b\i\u\tab\tx

where:

<SP> designates a space (ASCII value 0x20)

<CR> designates a carriage return (ASCII value 0x0d)

<LF> designates a line feed (ASCII value 0x0a)

After the dictionary is initialized, the writer MUST set the write offset and the end offset of the dictionary, as specified in section [2.1.3.1.4](#Section_a7c5162f7d864e14a75f043c94eb1307), to 207 (pointing to the byte that follows the pre-loaded string).

**Note**The dictionary will not be used when the value of the **COMPTYPE** field is set to UNCOMPRESSED, as specified in section [2.1.3.1.1](#Section_a1f226ed31e345659d26af3c6714c93f).

#### CRC

The writer MUST initialize the value of the **CRC** field, as specified in section [2.1.3.1.1](#Section_a1f226ed31e345659d26af3c6714c93f), which contains a [**cyclic redundancy check (CRC)**](#gt_9cb45a36-92bb-4c14-b2fd-2ad7e2979bfd), to zero.

##### CRC Lookup Table

The pre-computed table used for generating the value of the **CRC** field, as specified in section [2.1.3.1.1](#Section_a1f226ed31e345659d26af3c6714c93f), MUST contain the following 256 **DWORDs**. The **DWORD** type is specified in [[MS-DTYP]](%5BMS-DTYP%5D.pdf#Section_cca2742956894a16b2b49325d93e4ba2).

1. 0x00000000, 0x77073096, 0xee0e612c, 0x990951ba,
2. 0x076dc419, 0x706af48f, 0xe963a535, 0x9e6495a3,
3. 0x0edb8832, 0x79dcb8a4, 0xe0d5e91e, 0x97d2d988,
4. 0x09b64c2b, 0x7eb17cbd, 0xe7b82d07, 0x90bf1d91,
5. 0x1db71064, 0x6ab020f2, 0xf3b97148, 0x84be41de,
6. 0x1adad47d, 0x6ddde4eb, 0xf4d4b551, 0x83d385c7,
7. 0x136c9856, 0x646ba8c0, 0xfd62f97a, 0x8a65c9ec,
8. 0x14015c4f, 0x63066cd9, 0xfa0f3d63, 0x8d080df5,
9. 0x3b6e20c8, 0x4c69105e, 0xd56041e4, 0xa2677172,
10. 0x3c03e4d1, 0x4b04d447, 0xd20d85fd, 0xa50ab56b,
11. 0x35b5a8fa, 0x42b2986c, 0xdbbbc9d6, 0xacbcf940,
12. 0x32d86ce3, 0x45df5c75, 0xdcd60dcf, 0xabd13d59,
13. 0x26d930ac, 0x51de003a, 0xc8d75180, 0xbfd06116,
14. 0x21b4f4b5, 0x56b3c423, 0xcfba9599, 0xb8bda50f,
15. 0x2802b89e, 0x5f058808, 0xc60cd9b2, 0xb10be924,
16. 0x2f6f7c87, 0x58684c11, 0xc1611dab, 0xb6662d3d,
17. 0x76dc4190, 0x01db7106, 0x98d220bc, 0xefd5102a,
18. 0x71b18589, 0x06b6b51f, 0x9fbfe4a5, 0xe8b8d433,
19. 0x7807c9a2, 0x0f00f934, 0x9609a88e, 0xe10e9818,
20. 0x7f6a0dbb, 0x086d3d2d, 0x91646c97, 0xe6635c01,
21. 0x6b6b51f4, 0x1c6c6162, 0x856530d8, 0xf262004e,
22. 0x6c0695ed, 0x1b01a57b, 0x8208f4c1, 0xf50fc457,
23. 0x65b0d9c6, 0x12b7e950, 0x8bbeb8ea, 0xfcb9887c,
24. 0x62dd1ddf, 0x15da2d49, 0x8cd37cf3, 0xfbd44c65,
25. 0x4db26158, 0x3ab551ce, 0xa3bc0074, 0xd4bb30e2,
26. 0x4adfa541, 0x3dd895d7, 0xa4d1c46d, 0xd3d6f4fb,
27. 0x4369e96a, 0x346ed9fc, 0xad678846, 0xda60b8d0,
28. 0x44042d73, 0x33031de5, 0xaa0a4c5f, 0xdd0d7cc9,
29. 0x5005713c, 0x270241aa, 0xbe0b1010, 0xc90c2086,
30. 0x5768b525, 0x206f85b3, 0xb966d409, 0xce61e49f,
31. 0x5edef90e, 0x29d9c998, 0xb0d09822, 0xc7d7a8b4,
32. 0x59b33d17, 0x2eb40d81, 0xb7bd5c3b, 0xc0ba6cad,
33. 0xedb88320, 0x9abfb3b6, 0x03b6e20c, 0x74b1d29a,
34. 0xead54739, 0x9dd277af, 0x04db2615, 0x73dc1683,
35. 0xe3630b12, 0x94643b84, 0x0d6d6a3e, 0x7a6a5aa8,
36. 0xe40ecf0b, 0x9309ff9d, 0x0a00ae27, 0x7d079eb1,
37. 0xf00f9344, 0x8708a3d2, 0x1e01f268, 0x6906c2fe,
38. 0xf762575d, 0x806567cb, 0x196c3671, 0x6e6b06e7,
39. 0xfed41b76, 0x89d32be0, 0x10da7a5a, 0x67dd4acc,
40. 0xf9b9df6f, 0x8ebeeff9, 0x17b7be43, 0x60b08ed5,
41. 0xd6d6a3e8, 0xa1d1937e, 0x38d8c2c4, 0x4fdff252,
42. 0xd1bb67f1, 0xa6bc5767, 0x3fb506dd, 0x48b2364b,
43. 0xd80d2bda, 0xaf0a1b4c, 0x36034af6, 0x41047a60,
44. 0xdf60efc3, 0xa867df55, 0x316e8eef, 0x4669be79,
45. 0xcb61b38c, 0xbc66831a, 0x256fd2a0, 0x5268e236,
46. 0xcc0c7795, 0xbb0b4703, 0x220216b9, 0x5505262f,
47. 0xc5ba3bbe, 0xb2bd0b28, 0x2bb45a92, 0x5cb36a04,
48. 0xc2d7ffa7, 0xb5d0cf31, 0x2cd99e8b, 0x5bdeae1d,
49. 0x9b64c2b0, 0xec63f226, 0x756aa39c, 0x026d930a,
50. 0x9c0906a9, 0xeb0e363f, 0x72076785, 0x05005713,
51. 0x95bf4a82, 0xe2b87a14, 0x7bb12bae, 0x0cb61b38,
52. 0x92d28e9b, 0xe5d5be0d, 0x7cdcefb7, 0x0bdbdf21,
53. 0x86d3d2d4, 0xf1d4e242, 0x68ddb3f8, 0x1fda836e,
54. 0x81be16cd, 0xf6b9265b, 0x6fb077e1, 0x18b74777,
55. 0x88085ae6, 0xff0f6a70, 0x66063bca, 0x11010b5c,
56. 0x8f659eff, 0xf862ae69, 0x616bffd3, 0x166ccf45,
57. 0xa00ae278, 0xd70dd2ee, 0x4e048354, 0x3903b3c2,
58. 0xa7672661, 0xd06016f7, 0x4969474d, 0x3e6e77db,
59. 0xaed16a4a, 0xd9d65adc, 0x40df0b66, 0x37d83bf0,
60. 0xa9bcae53, 0xdebb9ec5, 0x47b2cf7f, 0x30b5ffe9,
61. 0xbdbdf21c, 0xcabac28a, 0x53b39330, 0x24b4a3a6,
62. 0xbad03605, 0xcdd70693, 0x54de5729, 0x23d967bf,
63. 0xb3667a2e, 0xc4614ab8, 0x5d681b02, 0x2a6f2b94,
64. 0xb40bbe37, 0xc30c8ea1, 0x5a05df1b, 0x2d02ef8d

### Processing Rules

#### RTF Compression Format

Unless otherwise specified, sizes in this section are expressed using the **BYTE** type, and multiple-byte values are stored in [**little-endian**](#gt_079478cb-f4c5-4ce5-b72b-2144da5d2ce7) format. The **BYTE** type is specified in [[MS-DTYP]](%5BMS-DTYP%5D.pdf#Section_cca2742956894a16b2b49325d93e4ba2).

##### RTF Compression ABNF Grammar

This section uses [**Augmented Backus-Naur Form (ABNF)**](#gt_24ddbbb4-b79e-4419-96ec-0fdd229c9ebf), as specified in [[RFC5234]](https://go.microsoft.com/fwlink/?LinkId=123096), to define the format of the contents stored in the **PidTagRtfCompressed** property ([[MS-OXPROPS]](%5BMS-OXPROPS%5D.pdf#Section_f6ab1613aefe447da49c18217230b148) section 2.941).

1. RTFCOMPRESSED=Header CONTENTS
2. Header=COMPSIZE RAWSIZE COMPTYPE CRC ; The size of the Header field is
 ; 16 (0x0010) bytes.
3. COMPSIZE =DWORD ; Writers MUST set the COMPSIZE field to
4. ; the length of the compressed data
5. ; (the CONTENTS field) in bytes
6. ; plus 12 (the count of the
7. ; remaining bytes from the header).
8. RAWSIZE =DWORD ; The size in bytes of the
 ; uncompressed content.
9. COMPTYPE=COMPRESSED / UNCOMPRESSED ; The type of compression.
10. COMPRESSED =%x4C.5A.46.75 ; Value of 0x75465A4C.
11. UNCOMPRESSED=%x4D.45.4C.41 ; Value of 0x414C454D.
12. CRC =DWORD ; If the COMPTYPE field is set to
13. ; COMPRESSED, then the CRC field is
14. ; computed from the CONTENTS field.
15. ; If the COMPTYPE field is set to
 ; UNCOMPRESSED, then the CRC field
16. ; MUST be set to %x00.00.00.00.
17. CONTENTS=RAWDATA / COMPRESSEDDATA ; The CONTENTS field is set
18. ; to RAWDATA if the COMPTYPE
19. ; field is set to UNCOMPRESSED.
20. ; The CONTENTS field is set
21. ; to COMPRESSEDDATA if the COMPTYPE
22. ; field is set to COMPRESSED.
23. RAWDATA=\*LITERAL
24. COMPRESSEDDATA=[\*RUN] ENDRUN [PADDING]
25. RUN=CONTROL 8\*8TOKEN
26. ENDRUN=CONTROL 1\*8TOKEN
27. CONTROL= OCTET
28. Token=REFERENCE / LITERAL
29. REFERENCE=WORD ; Value is in big-endian format.
30. LITERAL=OCTET
31. PADDING=\*OCTET

##### Compressed RTF

The content of the compressed [**RTF**](#gt_a9aa8673-7798-4eba-a048-8b7c95a7b080), as specified by the **RTFCOMPRESSED** field in section [2.1.3.1.1](#Section_a1f226ed31e345659d26af3c6714c93f), consists of a header and a series of runs. The number of runs varies based on the quantity of content that is compressed and sizes of the matches in the dictionary, as specified in section [2.1.2.1](#Section_4238b0e2714742da88c9ea45a1243e67), and illustrated in the following diagram.

| Header | RUN1 | RUN2 | RUN3 | RUN4 | ... | ENDRUN | PADDING |
| --- | --- | --- | --- | --- | --- | --- | --- |

The [**ABNF**](#gt_24ddbbb4-b79e-4419-96ec-0fdd229c9ebf) grammar specified in section 2.1.3.1.1 contains necessary details that are supplementary to the constructs defined in this section.

##### Compressed Run

A run is composed of a control byte and eight variable-sized tokens. A run is specified in section [2.1.3.1.1](#Section_a1f226ed31e345659d26af3c6714c93f) as the **RUN** field, and the control byte is specified in section 2.1.3.1.1 as the **CONTROL** field. The final run, as specified by the **ENDRUN** field in section 2.1.3.1.1, contains from one to eight tokens.

| CONTROL | TOKEN1 | TOKEN2 | TOKEN3 | TOKEN4 | TOKEN5 | TOKEN6 | TOKEN7 | TOKEN8 |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 1 Byte | Varies | Varies | Varies | Varies | Varies | Varies | Varies | Varies |

A token, as specified by the **Token** field in section 2.1.3.1.1, is either a dictionary reference or a literal, depending on the value of the corresponding bit in the control byte, as follows:

* If the bit in the **CONTROL** field is zero, the corresponding token is a 1-byte literal that represents the exact byte in the uncompressed content.
* If the bit in the **CONTROL** field is 1, the corresponding token is a 2-byte dictionary reference that indicates the offset and length of a series of bytes in the dictionary that corresponds to the bytes in the uncompressed content. For more details about dictionary references, see section [2.1.3.1.5](#Section_b12474dfe0ef47319315454a49a984d8).

Each control byte contains details about how to interpret the next eight tokens. The low bit (bitmask %x1) in the **CONTROL** field corresponds to Token1, the second bit (bitmask %x2) corresponds to Token2, and so on. In the **ENDRUN** field, the bits in the **CONTROL** field after the completion dictionary reference are undefined and MUST be ignored.

The length of a run can be computed from the control byte because each bit in the control byte that is set to zero represents a literal that is 1 byte long, and each bit in the control byte that is set to 1 represents a dictionary reference that is 2 bytes long. Therefore, the length of a run (except the final run) is as follows.

1. run\_length = 1 + (number of 0 bits) + (number of 1 bits) \* 2

##### Dictionary

This algorithm uses a dictionary that behaves as a 4096-byte circular array. When advancing a read or write position within the dictionary, a reference beyond the last index of the array wraps to a reference to the first byte and then advances from there.

The dictionary conceptually has a write offset, a read offset, and an end offset, all of which are zero-based unsigned values, as follows:

* Write offset: The index in the dictionary where the next byte is added.
* Read offset: The index in the dictionary from which the next byte is read.
* End offset: The number of bytes currently in the dictionary. It MUST be less than or equal to 4096.

The end offset is incremented until its value is 4096.

##### Dictionary Reference

A dictionary reference is a 16-bit packed structure stored in the value of the **REFERENCE** field, as specified in section [2.1.3.1.1](#Section_a1f226ed31e345659d26af3c6714c93f). The dictionary reference is stored in [**big-endian**](#gt_6f6f9e8e-5966-4727-8527-7e02fb864e7e) form on the wire. The format of this reference is as follows.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 20 | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 30 | 1 |
| Offset | Length |

**Offset (12 bits):** This field contains an index from the beginning of the dictionary that indicates where the matched content will start.

An offset that equals the write offset of the dictionary has the special meaning of completion of all compressed data, as specified in section [2.3.3.2](#Section_662579ba42794114b208848486e135dd), step 8. In this case, the writer MUST set the **Length** field to zero, and readers SHOULD ignore the **Length** field.

**Length (4 bits):** This value indicates the length of the matched content and is 2 bytes less than the actual length of the matched content.

#### Calculate a CRC from a Given Array of Bytes

Given an initial value of the **CRC** field, as specified in section [2.1.3.1.1](#Section_a1f226ed31e345659d26af3c6714c93f), or the value of the **CRC** field returned from a prior call (referred to in the following example as the **crcValue** field, which is a **DWORD** ([[MS-DTYP]](%5BMS-DTYP%5D.pdf#Section_cca2742956894a16b2b49325d93e4ba2))), the following is the algorithm for calculating the value of the **CRC** field for a given array of bytes (in pseudo-code). **tablePosition** is used as the index to get the value of **crcTableValue** from the **CRC Lookup Table**, as specified in section [2.1.2.2.1](#Section_2500f63ea1ec4605a80dd41ab63e80e9).

1. FOR each byte in the input array
2. SET tablePosition to (crcValue XOR byte) BITWISE-AND 0xff
3. SET intermediateValue to crcValue RIGHTSHIFTED by 8 bits
4. SET crcValue to (crcTableValue at position tablePosition)
5. XOR intermediateValue
6. ENDFOR
7. RETURN crcValue

## Decompression Algorithm Details

### Abstract Data Model

This section describes a conceptual model of possible data organization that an implementation maintains to participate in this algorithm. The described organization is provided to facilitate the explanation of how the algorithm behaves. This document does not mandate that implementations adhere to this model, as long as their external behavior is consistent with that described in this document.

The abstract data model specified in section [2.1.1](#Section_d7604c1e98f04b8bb91f051d3db228e1) also applies to decompression.

#### Input and Output

In this section, the input (the compressed [**RTF**](#gt_a9aa8673-7798-4eba-a048-8b7c95a7b080) data, including the header) and the output (the decompressed data) are treated as streams.

### Initialization

All initialization specified in section [2.1.2](#Section_ea1e702acbb349ffa7c519115749222e) is required by the decompression process, and therefore MUST be done.

#### Header

Before beginning decompression, the reader MUST read the **HEADER** field, as specified in section [2.1.3.1.1](#Section_a1f226ed31e345659d26af3c6714c93f). If the value of the **COMPTYPE** field, as specified in section 2.1.3.1.1, is any value other than COMPRESSED or UNCOMPRESSED, then the reader MUST treat the input stream as corrupt.

If the value of the **COMPTYPE** field is COMPRESSED, then the reader MUST decompress the stream by using the decompression algorithm specified in section [2.2.3.2](#Section_592e0b558b8645aeb9d1b4830e2969ea). If the value of the **COMPTYPE** field is UNCOMPRESSED, then the contents are uncompressed and the reader MUST copy the contents as-is to the output stream, as specified in section [2.2.3.1](#Section_20dbae84b3ef407a9e8b11f748c7d845).

#### Output

The output stream MUST initially have a length of zero.

### Processing Rules

If the decompression process, as defined in section [2.2](#Section_2ab4a791b8ef42c7876a859c3e9d8970), terminates prior to the end of the input, then the remainder of the input (the **PADDING** field, as specified in section [2.1.3.1.1](#Section_a1f226ed31e345659d26af3c6714c93f),) MUST be included in the value of the **CRC** field, as specified in section 2.1.3.1.1. After this is done, if the computed value of the **CRC** field does not equal that which is specified in the **CRC** field of the header, then the reader MUST treat the input as corrupt.

#### Decompressing Input of COMPTYPE UNCOMPRESSED

When the **COMPTYPE** field is set to UNCOMPRESSED, the reader SHOULD read all bytes until the end of the stream is reached, regardless of the value of the **RAWSIZE** field. Or, the reader MAY read the number of bytes specified by the **RAWSIZE** field from the input (the **Header** field) and write them to the output. The **COMPTYPE**, **RAWSIZE** and **Header** fields are specified in section [2.1.3.1.1](#Section_a1f226ed31e345659d26af3c6714c93f).

The reader MUST NOT validate the value of the **CRC** field.

#### Decompressing Input of COMPTYPE COMPRESSED

If at any point during the steps specified in this section, the end of the input is reached before the termination of decompression, then the reader MUST treat the input as corrupt.

When the **COMPTYPE** field is set to COMPRESSED, the decompression process is a straightforward loop, as follows:

* Read the **CONTROL** field, as specified in section [2.1.3.1.1](#Section_a1f226ed31e345659d26af3c6714c93f), from the input.
* Starting with the lowest bit (the 0x01 bit) in the **CONTROL** field, test each bit and carry out the actions as follows.
* After all bits in the **CONTROL** field have been tested, read another value of a **CONTROL** field from the input and repeat the bit-testing process.

For each bit, the reader MUST evaluate its value and complete the corresponding steps as specified in this section.

If the value of the bit is zero:

1. Read a 1-byte literal from the input and write it to the output.
2. Set the byte in the dictionary at the current write offset to the literal from step 1.
3. Increment the write offset and update the end offset, as appropriate, as specified in section [2.1.3.1.4](#Section_a7c5162f7d864e14a75f043c94eb1307).

If the value of the bit is 1:

1. Read a 16-bit dictionary reference from the input in [**big-endian**](#gt_6f6f9e8e-5966-4727-8527-7e02fb864e7e) byte-order.
2. Extract the offset from the dictionary reference, as specified in section [2.1.3.1.5](#Section_b12474dfe0ef47319315454a49a984d8).
3. Compare the offset to the dictionary's write offset. If they are equal, then the decompression is complete; exit the decompression loop. If they are not equal, continue to the next step.
4. Set the dictionary's read offset to offset.
5. Extract the length from the dictionary reference and calculate the actual length by adding 2 to the length that is extracted from the dictionary reference.
6. Read a byte from the current dictionary read offset and write it to the output.
7. Increment the read offset, wrapping as appropriate, as specified in section 2.1.3.1.4.
8. Write the byte to the dictionary at the write offset.
9. Increment the write offset and update the end offset, as appropriate, as specified in section 2.1.3.1.4.
10. Continue from step 6 until the number of bytes calculated in step 5 has been read from the dictionary.

The input value of the **CRC** field, as specified in section 2.1.3.1.1, MUST be calculated from every byte in the **CONTENTS** field, per the process specified in section [2.1.3.2](#Section_a395d09082f64ac085c4057678b2c8e8). After the decompression process, if the calculated value of the **CRC** field does not match the value of the **CRC** field in the header, then the reader MUST treat the input as corrupt.

## Compression Algorithm Details

### Abstract Data Model

This section describes a conceptual model of possible data organization that an implementation maintains to participate in this algorithm. The described organization is provided to facilitate the explanation of how the algorithm behaves. This document does not mandate that implementations adhere to this model as long as their external behavior is consistent with that described in this document.

The abstract data model specified in section [2.1.1](#Section_d7604c1e98f04b8bb91f051d3db228e1) also applies to compression.

#### Input and Output

For the purpose of this section, the input (the uncompressed [**RTF**](#gt_a9aa8673-7798-4eba-a048-8b7c95a7b080) data) and the output (the compressed data) will be treated as in-memory buffers of appropriate sizes. The output has an output cursor, which defines where the next byte of the output is written. The input has an input cursor, which defines the position from which the next byte of input is read.

#### Run Information

Compressing data when the value of the **COMPTYPE** field, as specified in section [2.1.3.1.1](#Section_a1f226ed31e345659d26af3c6714c93f), is COMPRESSED is most easily understood and implemented if the writer does so one run at a time, writing each run to the output as it is completed. Information stored for a run includes:

* The current control byte (the **CONTROL** field, as specified in section 2.1.3.1.1) for the run, represented as a **BYTE** ([[MS-DTYP]](%5BMS-DTYP%5D.pdf#Section_cca2742956894a16b2b49325d93e4ba2)).
* A mask (called the control bit), represented as a **BYTE**. The writer uses the control bit to write to the control byte, as specified in section [2.3.3.2](#Section_662579ba42794114b208848486e135dd).
* A token buffer, 16 bytes in length.
* The offset, in bytes, into the token buffer (the "token offset"), representing the next position in the buffer to which a token will be written.

In the implementation specified in the remainder of section [2.3](#Section_c2da31d8797047daac2fc74c8f1e4056), a run is considered completed when the value of the control bit is 0x80 after a token has been written.

### Initialization

All initialization specified in section [2.1.2](#Section_ea1e702acbb349ffa7c519115749222e) is required by the compression process, and therefore MUST be done.

#### Input and Output

The writer MUST set the input cursor to the first byte in the input buffer.

The writer MUST set the output cursor to the 17th byte (to make space for the compressed header).

### Processing Rules

#### Compressing a Buffer of Uncompressed Contents with COMPTYPE UNCOMPRESSED

When the **COMPTYPE** field, as specified in section [2.1.3.1.1](#Section_a1f226ed31e345659d26af3c6714c93f), is set to UNCOMPRESSED, the writer MUST copy the uncompressed contents from the input buffer to the output buffer starting at the current output cursor. Compression MUST continue by filling in the header, as specified in section [2.3.3.1.1](#Section_a77ef978ff5846b3857d365bbd9b9e5a).

The writer SHOULD NOT compute the value of the **CRC** field and MUST set the value of the **CRC** field in the header to 0x00000000. The **CRC** field is specified in section 2.1.3.1.1.

##### Filling in the Header

Using the fields defined in the [**RTF**](#gt_a9aa8673-7798-4eba-a048-8b7c95a7b080) compression [**ABNF**](#gt_24ddbbb4-b79e-4419-96ec-0fdd229c9ebf) grammar, specified in section [2.1.3.1.1](#Section_a1f226ed31e345659d26af3c6714c93f), the writer MUST fill in the header by using the following process:

1. Set the **COMPSIZE** field of the header to the length of the **CONTENTS** field in the output buffer plus 12.
2. Set the value of the **RAWSIZE** field of the header to the number of bytes read from the input.
3. Set the value of the **COMPTYPE** field of the header to UNCOMPRESSED.
4. Set the value of the **CRC** field of the header to zero.

#### Compressing a Buffer of Uncompressed Contents with COMPTYPE COMPRESSED

When the **COMPTYPE** field is set to COMPRESSED, compression proceeds as a loop, as follows:

1. The writer MUST (re)initialize the run by setting its control byte to zero, its control bit to 0x01, and its token offset to zero.
2. If there is no more input, then the writer MUST exit the compression loop (by advancing to step 8).
3. Locate the longest match in the dictionary for the current input cursor, as specified in section [2.3.3.2.1](#Section_eb4b209bf2f04876a28b1cfa1827423c).
4. If the match is zero or 1 byte in length, then the writer MUST copy the literal at the input cursor to the run's token buffer at token offset. The writer MUST increment the token offset and the input cursor.
5. If the match is 2 bytes or longer, then the writer MUST create a dictionary reference, as specified in section [2.1.3.1.5](#Section_b12474dfe0ef47319315454a49a984d8), from the offset of the match and the length. (**Note**: The value stored in the **Length** field, as specified in section 2.1.3.1.5, is length minus 2). The writer MUST insert this dictionary reference in the token buffer as a [**big-endian**](#gt_6f6f9e8e-5966-4727-8527-7e02fb864e7e) word at the current token offset. The control bit MUST be bitwise ORed into the control byte, thus setting the bit that corresponds to the current token to 1. The writer MUST advance the token offset by 2 bytes and MUST advance the input cursor by the length of the match.
6. If the control bit is not 0x80, then the control bit MUST be left-shifted by one bit and compression MUST continue building the run by returning to step 2.
7. If the control bit is equal to 0x80, then the writer MUST write the run to the output by writing the BYTE control byte, and then copying the token offset number of bytes from the token buffer to the output. The writer MUST advance the output cursor by the token offset plus 1 byte. Continue with compression by returning to step 1.
8. A dictionary reference MUST be created from an offset equal to the current write offset of the dictionary and a length of zero, and inserted in the token buffer as a big-endian word at the current token offset. The writer MUST then advance the token offset by 2 bytes. The control bit MUST be ORed into the control byte, thus setting the bit that corresponds to the current token to 1. When compressing zero bytes of data, the writer adds a null value during compression and the compressed run will be "02 00 0D 00" instead of "01 0C F0".
9. The writer MUST write the current run to the output by writing the value of the **CONTROL** field, as specified in section [2.1.3.1.1](#Section_a1f226ed31e345659d26af3c6714c93f), and then copying the token offset number of bytes from the token buffer to the output. The output cursor is advanced by the token offset plus 1 byte.

After the output has been completed by execution of step 9, the writer MUST complete the output by filling the header, as specified in section [2.3.3.2.2](#Section_4c589b4d6334418e93fd1c75f820e770).

The writer MUST calculate the value of the **CRC** field for every byte written to the **CONTENTS** field, as specified in section 2.1.3.1.1, and set the value of the **CRC** field of the header.

##### Finding the Longest Match to Input

The purpose here is to scan over the dictionary to locate the longest string. It is important that, as the code finds a new longest match, the newly matched character SHOULD be added to the dictionary at that time (refer to the **AddByteToDictionary** procedure calls in the pseudo-code as follows).

In the case where the length of the match is zero, the literal that is being searched for MUST be added to the dictionary.

The scan MUST begin at the dictionary write offset plus 1 when the dictionary end offset is equal to 4096 bytes. When the end offset is less than 4096 bytes, the scan MUST begin at index zero. The scan SHOULD stop when 17 characters are matched but MUST stop after the finalOffset position is scanned, where finalOffset is defined as the dictionary write offset modulo 4096.

Matches that start at or before finalOffset and match across finalOffset allow a repeating sequence of characters, such as "XYZXYZXYZXYZ", to be represented as a series of appropriate initial literals ('X' 'Y' 'Z') and a single dictionary reference. (This example generates an offset of 210 and a length of 9, assuming that the dictionary is initialized as specified in section [2.1.2.1](#Section_4238b0e2714742da88c9ea45a1243e67).) For a more detailed example, see section [3.2.2](#Section_59eb3a356ee14a0893b9b9f4a7e3a0ca).

The algorithm computes the longest match in the dictionary of the current position within the input by using one of multiple implementation-dependent mechanisms. The following pseudocode is provided as one example; however, it is not necessary to follow this exactly, so long as the decompression algorithm specified in section [2.2](#Section_2ab4a791b8ef42c7876a859c3e9d8970) generates the original input given the compressed output generated.

1. PROCEDURE FindLongestMatch
2. SET finalOffset to the Write Offset of the Dictionary modulo 4096
3. IF the Dictionary's End Offset is not equal to the Dictionary buffer size THEN
4. SET matchOffset to 0
5. ELSE
6. SET matchOffset to (the Dictionary's Write Offset + 1) modulo 4096
7. ENDIF
8. SET bestMatchLength to 0
9. REPEAT
10. CALL TryMatch with matchOffset and the Input Cursor
11. SET matchOffset to (matchOffset + 1) modulo 4096
12. UNTIL matchOffset equals finalOffset
13. OR until bestMatchLength is 17 bytes long
14. IF bestMatchLength is 0 THEN
15. CALL AddByteToDictionary with the byte at Input Cursor
16. ENDIF
17. RETURN offset of bestMatchOffset and bestMatchLength
18. ENDPROCEDURE
19. PROCEDURE TryMatch
20. SET maxLength to the minimum of 17 and remaining bytes of Input
21. SET matchLength to 0
22. SET inputOffset to the Input Cursor
23. SET dictionaryOffset to matchOffset
24. WHILE matchLength is less than maxLength AND
25. the byte in the Dictionary at dictionaryOffset is equal to
26. the byte in Input at the inputOffset
27. INCREMENT matchLength
28. IF matchLength is greater than bestMatchLength THEN
29. CALL AddByteToDictionary with the byte
30. in Input at the inputOffset
31. ENDIF
32. INCREMENT inputOffset
33. SET dictionaryOffset to (dictionaryOffset + 1) modulo 4096
34. ENDWHILE
35. IF matchLength is greater than bestMatchLength THEN
36. SET bestMatchOffset to matchOffset
37. SET bestMatchLength to matchLength
38. ENDIF
39. ENDPROCEDURE
40. PROCEDURE AddByteToDictionary
41. SET the byte at the Dictionary's current Write Offset to the provided byte
42. IF the Dictionary's End Offset is less than the buffer size
43. THEN INCREMENT the End Offset
44. ENDIF
45. SET the Dictionary's Write Offset to
46. (the Dictionary's Write Offset + 1) modulo 4096
47. ENDPROCEDURE

##### Filling in the Header

Using the fields defined in the [**RTF**](#gt_a9aa8673-7798-4eba-a048-8b7c95a7b080) compression [**ABNF**](#gt_24ddbbb4-b79e-4419-96ec-0fdd229c9ebf) grammar, as specified in section [2.1.3.1.1](#Section_a1f226ed31e345659d26af3c6714c93f), the writer MUST fill in the header by using the following process:

1. Set the **COMPSIZE** field of the header to the number of **CONTENTS** bytes in the output buffer plus 12.
2. Set the **RAWSIZE** field of the header to the number of bytes read from the input.
3. Set the **COMPTYPE** field of the header to COMPRESSED.
4. Set the **CRC** field of the header to the value of the **CRC** field generated from the **CONTENTS** field. The value of the **CRC** field, as specified in section 2.1.3.1.1, MUST be calculated from every byte in the **CONTENTS** field by using the process specified in section [2.1.3.2](#Section_a395d09082f64ac085c4057678b2c8e8).

# Algorithm Examples

## Decompressing Compressed RTF

In the following examples, the compressed [**RTF**](#gt_a9aa8673-7798-4eba-a048-8b7c95a7b080) is examined in terms of "runs" for ease of exposition, where the term "run" refers to a control byte and the tokens that it represents. The length of a run can be computed as specified in section [2.1.3.1.3](#Section_8c192feae2ce450c9fb8b099b65cef44).

### Example 1: Simple Compressed RTF

#### Compressed RTF Data

1. 000000: 2d 00 00 00 2b 00 00 00-4c 5a 46 75 f1 c5 c7 a7
2. 000010: 03 00 0a 00 72 63 70 67-31 32 35 42 32 0a f3 20
3. 000020: 68 65 6c 09 00 20 62 77-05 b0 6c 64 7d 0a 80 0f
4. 000030: a0

#### Compressed RTF Header

The first 16 bytes comprise the compressed [**RTF**](#gt_a9aa8673-7798-4eba-a048-8b7c95a7b080) header.

1. 000000: 2d 00 00 00 2b 00 00 00-4c 5a 46 75 f1 c5 c7 a7
2. COMPSIZE : 0x2d
3. RAWSIZE : 0x2b
4. COMPTYPE : COMPRESSED ; 0x75465a4c
5. CRC: 0xa7c7c5f1

#### Initialization

The dictionary is initialized with the data, as described in section [2.1.2.1](#Section_4238b0e2714742da88c9ea45a1243e67). After the initialization, the dictionary is as follows.

1. WritePosition: 207
2. 0 1 2 3 4 5 6
3. 01234567890123456789012345678901234567890123456789012345678901234
4. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
5. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
6. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
7. 0195: b\i\u\tab\tx
8. Nonprintable characters:
9. Position:0168 Byte:0x0d
10. Position:0169 Byte:0x0a

#### Run 1

The first run begins on byte 16. The value of the **CONTROL** field, as described in section [2.1.3.1.1](#Section_a1f226ed31e345659d26af3c6714c93f), at that location is 0x03. Represented as bits, the value of the **CONTROL** field would be %b00000011. The **CONTROL** field determines a run length, based on the number of '1' and '0' (zero) bits. Run length is equal to the number of '1' bits times 2 plus the number of '0' (zero) bits plus 1 for the **CONTROL** field itself. With a value of 0x3 for the **CONTROL** field, the run length is 11 bytes.

1. 000010: 03 00 0a 00 72 63 70 67 31 32 35

Because the low-order bit in the **CONTROL** is a 1, the first token in the run is a dictionary reference and consists of the two bytes 00 and 0a. Reading these into a **WORD** data type ([[MS-DTYP]](%5BMS-DTYP%5D.pdf#Section_cca2742956894a16b2b49325d93e4ba2)) in [**big-endian**](#gt_6f6f9e8e-5966-4727-8527-7e02fb864e7e) order, the dictionary reference is 0x000a. As described in section [2.1.3.1.5](#Section_b12474dfe0ef47319315454a49a984d8), the offset into the dictionary is the upper 12 bits (for example, 0), and the length is the lower 4 bits (for example, 0xa). The length is stored as 2 less than the actual length, so 2 is added to the length, making the actual length 0x0C (12). Reading 12 bytes from the dictionary at offset zero returns the content "{\rtf1\ansi\".

1. 0 1 2 3 4 5 6
2. 01234567890123456789012345678901234567890123456789012345678901234
3. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi

This content is copied to the output buffer and written to the write location for the dictionary. The new dictionary is as follows.

1. WritePosition: 219
2. 0 1 2 3 4 5 6
3. 01234567890123456789012345678901234567890123456789012345678901234
4. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
5. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
6. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
7. 0195: b\i\u\tab\tx{\rtf1\ansi\
8. Nonprintable characters:
9. Position:0168 Byte:0x0d
10. Position:0169 Byte:0x0a

The output stream is now as follows.

"{\rtf1\ansi\"

The next control bit is 1 (%b000000**1**1), specifying another dictionary reference for the bytes for which are 00 and 72. Converting to a **WORD** data type results in 0x0072, and extracting the offset and length results in offset equal to 0x0007, and a length of 0x4 (0x2+2).

Looking up the dictionary position 7 for 4 bytes results in: "ansi".

1. 0 1 2 3 4 5 6
2. 01234567890123456789012345678901234567890123456789012345678901234
3. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi

This extracted content is appended to the output buffer and to the dictionary. The new dictionary is as follows.

1. WritePosition: 223
2. 0 1 2 3 4 5 6
3. 01234567890123456789012345678901234567890123456789012345678901234
4. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
5. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
6. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
7. 0195: b\i\u\tab\tx{\rtf1\ansi\ansi
8. Nonprintable characters:
9. Position:0168 Byte:0x0d
10. Position:0169 Byte:0x0a

The output stream is now as follows.

"{\rtf1\ansi\ansi"

The next control bit is 0 (%b00000**0**11), specifying a literal byte token. That token value is 0x63. Because it is a literal, no dictionary lookup happens. The byte is appended to the dictionary and to the output stream.

The new dictionary is as follows.

1. WritePosition: 224
2. 0 1 2 3 4 5 6
3. 01234567890123456789012345678901234567890123456789012345678901234
4. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
5. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
6. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
7. 0195: b\i\u\tab\tx{\rtf1\ansi\ansic
8. Nonprintable characters:
9. Position:0168 Byte:0x0d
10. Position:0169 Byte:0x0a

The output stream is now as follows.

"{\rtf1\ansi\ansic"

The next control bit is 0 (%b0000**0**011), specifying another literal byte token. That token value is 0x70. Because it is a literal, no dictionary lookup happens. The byte is appended to the dictionary and the output stream.

The new dictionary is as follows.

1. WritePosition: 225
2. 0 1 2 3 4 5 6
3. 01234567890123456789012345678901234567890123456789012345678901234
4. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
5. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
6. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
7. 0195: b\i\u\tab\tx{\rtf1\ansi\ansicp
8. Nonprintable characters:
9. Position:0168 Byte:0x0d
10. Position:0169 Byte:0x0a

The output stream is now as follows.

"{\rtf1\ansi\ansicp"

Repeating for the remaining tokens in the run, the following bytes are added to the dictionary and the output stream (67 31 32 35).

The new dictionary is as follows.

1. WritePosition: 229
2. 0 1 2 3 4 5 6
3. 01234567890123456789012345678901234567890123456789012345678901234
4. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
5. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
6. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
7. 0195: b\i\u\tab\tx{\rtf1\ansi\ansicpg125
8. Nonprintable characters:
9. Position:0168 Byte:0x0d
10. Position:0169 Byte:0x0a

The output stream is now as follows.

"{\rtf1\ansi\ansicpg125"

The entire **CONTROL** field is now processed and the first run is now evaluated.

#### Run 2

The next run is now loaded and the same logic as described in Run 1 is executed.

RunSize: 11 bytes

1. 00001b: 42 32 0a f3 20 68 65 6c 09 00 20

| Bytes | Description |
| --- | --- |
| 42 | Control byte: 0x42Bits: %b01000010 |
| 32 | '2' |
| 0a f3 | Dictionary reference: 0af3Offset: 0x0af (175)Length: [0x3+2] (5)Content: "\pard" |
| 20 | ' ' |
| 68 | 'h' |
| 65 | 'e' |
| 6c | 'l' |
| 09 00 | Dictionary reference: 0900Offset: 0x090 (144)Length: [0x0+2] (2)Content: "lo" |
| 20 | ' ' |

Dictionary:

1. WritePosition: 242
2. 0 1 2 3 4 5 6
3. 01234567890123456789012345678901234567890123456789012345678901234
4. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
5. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
6. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
7. 0195: b\i\u\tab\tx{\rtf1\ansi\ansicpg1252\pard hello
8. Nonprintable characters:
9. Position:0168 Byte:0x0d
10. Position:0169 Byte:0x0a

OutputStream:

"{\rtf1\ansi\ansicpg1252\pard hello "

#### Run 3

The final run is 11 bytes, as follows.

1. 000026: 62 77 05 b0 6c 64 7d 0a 80 0f a0

| Bytes | Description |
| --- | --- |
| 62 | Control byte: 0x62Bits: %b01100010 |
| 77 | 'w' |
| 05 b0 | Dictionary reference: 05b0Offset: 0x05b (91)Length: [0x0+2] (2)Content: "or" |
| 6c | 'l' |
| 64 | 'd' |
| 7d | '}' |
| 0a 80 | Dictionary reference: 0a80Offset: 0x0a8 (168)Length: [0x0+2] (2)Content: 0x0d 0x0a |
| 0f a0 | Dictionary reference: 0fa0Offset: 0x0fa (250)Length: [0x0+2] (2)Content: <END> |

The final dictionary reference is unique. The offset of 250 exactly matches the value of the **WritePosition** field at the time that the dictionary reference is encountered. This is an indicator that the end of the compressed content has been reached and decompression has to stop.

The final dictionary is as follows.

1. WritePosition: 250
2. 0 1 2 3 4 5 6
3. 01234567890123456789012345678901234567890123456789012345678901234
4. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
5. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
6. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
7. 0195: b\i\u\tab\tx{\rtf1\ansi\ansicpg1252\pard hello world}\_\_
8. Nonprintable characters:
9. Position:0168 Byte:0x0d
10. Position:0169 Byte:0x0a
11. Position:0248 Byte:0x0d
12. Position:0249 Byte:0x0a

The final decompressed output is as follows.

"{\rtf1\ansi\ansicpg1252\pard hello world}<CR><LF>"

### Example 2: Reading a Token from the Dictionary that Crosses WritePosition

The following example illustrates that the requirement that bytes be added to the dictionary as they are copied to the output is necessary to allow longer matches than would otherwise be possible.

#### Compressed RTF

1. 000000: 1a 00 00 00 1c 00 00 00-4c 5a 46 75 e2 d4 4b 51
2. 000010: 41 00 04 20 57 58 59 5a-0d 6e 7d 01 0e b0

#### Compressed RTF Header

1. 000000: 1a 00 00 00 1c 00 00 00-4c 5a 46 75 e2 d4 4b 51
2. COMPSIZE : 0x1a
3. RAWSIZE : 0x1c
4. COMPTYPE : COMPRESSED ; 0x75465a4c
5. CRC: 0x514bd4e2

#### Initialization

The dictionary is initialized with the data, as described in section [2.1.2.1](#Section_4238b0e2714742da88c9ea45a1243e67). After the initialization, the dictionary is as follows.

1. WritePosition: 207
2. 0 1 2 3 4 5 6
3. 01234567890123456789012345678901234567890123456789012345678901234
4. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
5. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
6. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
7. 0195: b\i\u\tab\tx
8. Nonprintable characters:
9. Position:0168 Byte:0x0d
10. Position:0169 Byte:0x0a

#### Run 1

The first run is 11 bytes long.

1. 000010: 41 00 04 20 57 58 59 5a 0d 6e 7d

| Bytes | Description |
| --- | --- |
| 41 | Control byte: 0x41Bits: %b01000001 |
| 00 04 | Dictionary reference: 0004Offset: 0x000 (0)Length: [0x4+2](6)Content: "{\rtf1" |
| 20 | ' ' |
| 57 | 'W' |
| 58 | 'X' |
| 59 | 'Y' |
| 5a | 'Z' |
| 0d 6e  | Dictionary reference: 0d6eOffset: 0x0d6 (214)Length: [0xe+2](16)Content: "WXYZWXYZWXYZWXYZ" |
| 7d | '}' |

After the first dictionary reference and the first five literal tokens are processed, the dictionary is as follows.

1. WritePosition: 218
2. 0 1 2 3 4 5 6
3. 01234567890123456789012345678901234567890123456789012345678901234
4. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
5. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
6. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
7. 0195: b\i\u\tab\tx{\rtf1 WXYZ
8. Nonprintable characters:
9. Position:0168 Byte:0x0d
10. Position:0169 Byte:0x0a

The output is now as follows.

"{\rtf1 WXYZ"

1. 000018:0d 6e 7d

The next token in the input is a dictionary reference at offset 214 and length 16. There are only 4 bytes in the dictionary following that offset. As each byte of the dictionary reference is copied to the output, it is also added to the dictionary. Therefore, after the first four bytes of the dictionary reference are copied, the dictionary is as follows.

1. WritePosition: 222
2. 0 1 2 3 4 5 6
3. 01234567890123456789012345678901234567890123456789012345678901234
4. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
5. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
6. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
7. 0195b\i\u\tab\tx{\ref1 WXYZWXYZ
8. Nonprintable characters:
9. Position:0168 Byte:0x0d
10. Position:0169 Byte:0x0a

The offset from which the dictionary reference is being copied has now been advanced from 214 to 218, which points to the newly written bytes, so the expansion continues with those bytes. The full expansion of the dictionary reference leads to a dictionary of the following.

1. WritePosition: 234
2. 0 1 2 3 4 5 6
3. 01234567890123456789012345678901234567890123456789012345678901234
4. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
5. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
6. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
7. 0195b\i\u\tab\tx{\ref1 WXYZWXYZWXYZWXYZWXYZ
8. Nonprintable characters:
9. Position:0168 Byte:0x0d
10. Position:0169 Byte:0x0a

The output is as follows.

"{\ref1 WXYZWXYZWXYZWXYZWXYZ"

There is one more literal token in this run, as follows.

1. 00001a: 7d

When decoded, this token leads to a dictionary of the following.

1. WritePosition: 235
2. 0 1 2 3 4 5 6
3. 01234567890123456789012345678901234567890123456789012345678901234
4. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
5. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
6. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
7. 0195: b\i\u\tab\tx{\ref1 WXYZWXYZWXYZWXYZWXYZ}
8. Nonprintable characters:
9. Position:0168 Byte:0x0d
10. Position:0169 Byte:0x0a

The output is as follows.

"{\ref1 WXYZWXYZWXYZWXYZWXYZ}"

#### Run 2

This run is only 3 bytes, as follows.

1. 00001b: 01 0e b0

| Bytes | Description |
| --- | --- |
| 01 | Control byte: 0x01Bits: %b00000001 |
| 0e b0 | Dictionary reference: 0004Offset: 0x0eb(235)Length: [0x0+2](2)Content: <END> |

Because the offset of the dictionary reference is equal to the current value of the **WritePosition** field, this indicates that the decompression is complete.

## Generating Compressed RTF

### Example 1: Simple RTF

This example compresses the following [**RTF**](#gt_a9aa8673-7798-4eba-a048-8b7c95a7b080) data.

"{\rtf1\ansi\ansicpg1252\pard hello world}<CR><LF>"

#### Initialization

The dictionary is initialized with the data, as described in section [2.3.2.1](#Section_de37d28fe4a84bbb9121704fb5d6e257). After the initialization, the dictionary is as follows.

1. WritePosition: 207
2. 0 1 2 3 4 5 6
3. 01234567890123456789012345678901234567890123456789012345678901234
4. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
5. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
6. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
7. 0195: b\i\u\tab\tx
8. Nonprintable characters:
9. Position:0168 Byte:0x0d
10. Position:0169 Byte:0x0a

CRC: 0

COMPSIZE: 0x000C

COMPTYPE: 0x75465a4c

The output is as follows.

1. Output cursor: 0x10
2. 000000: 00 00 00 00 00 00 00 00-4c 5a 46 75 00 00 00 00
3. 000010: 00 00 00 00 00 00 00 00-00 00 00 00 00 00 00 00
4. 000020: 00 00 00 00 00 00 00 00-00 00 00 00 00 00 00 00
5. 000030: 00 00 00 00 00 00 00 00-00 00 00 00 00 00 00 00

InputCursor is: 0 (zero)

#### Run 1

Start by initializing the following run information.

1. Control byte: 0x00
2. Control bit: 0x01
3. Token offset: 0x00
4. Token buffer: 00 00 00 00 00 00 00 00-00 00 00 00 00 00 00 00

Input data is "{\rtf1\ansi\ansicpg1252\pard hello world}<CR><LF>".

The dictionary is now scanned starting at index zero, looping until through index 207, in an attempt to find the largest match of the input data.

The first match starts at position zero. As each new byte is matched, the byte is copied to the dictionary write index and the write index is incremented. This match stops at byte 12. The maximum length match is stored as 12 before moving to the next character. No larger match is found. Because the match is greater than one character, a dictionary reference has to be written to the output (length is encoded as match length minus 2). The dictionary reference written to the output is offset = 0, length = 10, 0x000A.

The **CONTROL** field, as described in section [2.1.3.1.1](#Section_a1f226ed31e345659d26af3c6714c93f), sets the value at the control bit set to 1 and advances the control bit to the next token.

The run information is now as follows.

1. Control byte: 0x01
2. Control bit: 0x02
3. Token offset: 0x02
4. Token buffer: 00 0a 00 00 00 00 00 00-00 00 00 00 00 00 00 00

The dictionary is now as follows.

1. WritePosition: 219
2. 0 1 2 3 4 5 6
3. 01234567890123456789012345678901234567890123456789012345678901234
4. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
5. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
6. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
7. 0195: b\i\u\tab\tx{\rtf1\ansi\
8. Nonprintable characters:
9. Position:0168 Byte:0x0d
10. Position:0169 Byte:0x0a

The input data is now: "ansicpg1252\pard hello world}<CR><LF>".

Scanning the dictionary from index zero to index 219, new matches are calculated.

The first match is located at index 7. As each character is matched, it is moved to the dictionary write index. The match length is 4. No other larger match is located, and because the length is greater than one character, a dictionary reference is written to the output buffer (length is encoded as match length minus 2). The dictionary reference written to the output is offset = 7, length = 2, 0x0072.

The control bit location in the **CONTROL** field is set to 1, and the control bit is advanced.

The run information is now as follows.

1. Control byte: 0x03
2. Control bit: 0x04
3. Token offset: 0x04
4. Token buffer: 00 0a 00 72 00 00 00 00-00 00 00 00 00 00 00 00

The dictionary is now as follows.

1. WritePosition: 223
2. 0 1 2 3 4 5 6
3. 01234567890123456789012345678901234567890123456789012345678901234
4. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
5. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
6. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
7. 0195: b\i\u\tab\tx{\rtf1\ansi\ansi
8. Nonprintable characters:
9. Position:0168 Byte:0x0d
10. Position:0169 Byte:0x0a

The input data is now: "cpg1252\pard hello world}<CR><LF>".

Scanning the dictionary from index zero to index 223, new matches are located.

The first match is located at index 14. The 'c' character is matched, and is moved to the dictionary write index. The largest match is now 1 character. Continuing scanning, matches are located at positions 80 and 142, but because the match is not any larger, no additional characters are copied to the dictionary. Because the match is less than 2, a literal is written to the output stream.

The control bit location in the **CONTROL** field is set to zero and the control bit is advanced. The value of the **CONTROL** field is still 0x3 (%b00000011).

The run information is now as follows.

1. Control byte: 0x03
2. Control bit: 0x08
3. Token offset: 0x05
4. Token buffer: 00 0a 00 72 63 00 00 00-00 00 00 00 00 00 00 00

The dictionary is now as follows.

1. WritePosition: 224
2. 0 1 2 3 4 5 6
3. 01234567890123456789012345678901234567890123456789012345678901234
4. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
5. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
6. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
7. 0195: b\i\u\tab\tx{\rtf1\ansi\ansic
8. Nonprintable characters:
9. Position:0168 Byte:0x0d
10. Position:0169 Byte:0x0a

The input data is now: "pg1252\pard hello world}<CR><LF>".

Scanning the dictionary from index zero to index 224, new matches are located.

The first match is located at index 83. The 'p' character is matched, and is moved to the dictionary write index. The largest match is now 1 character. Continuing scanning, matches are located at positions 171, 176, and 181, but because the match is not any larger, no additional characters are copied to the dictionary. Because the match is less than 2, a literal is written to the output stream.

The control bit location in the **CONTROL** field is set to zero and the control bit is advanced.

The run information is now as follows.

1. Control byte: 0x03
2. Control bit: 0x10
3. Token offset: 0x06
4. Token buffer: 00 0a 00 72 63 70 00 00-00 00 00 00 00 00 00 00

The dictionary is now as follows.

1. WritePosition: 225
2. 0 1 2 3 4 5 6
3. 01234567890123456789012345678901234567890123456789012345678901234
4. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
5. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
6. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
7. 0195: b\i\u\tab\tx{\rtf1\ansi\ansicp
8. Nonprintable characters:
9. Position:0168 Byte:0x0d
10. Position:0169 Byte:0x0a

The input data is now: "g1252\pard hello world}<CR><LF>".

Scanning the dictionary from index zero to index 225, new matches are located.

The first match is located at index 156. The 'g' character is matched, and is moved to the dictionary write index. The largest match is now 1 character. Continuing scanning, matches are not found at any other locations. Because the match length is less than 2, a literal is written to the output stream.

The control bit location in the **CONTROL** field is set to zero and the control bit is advanced.

The run information is now as follows.

1. Control byte: 0x03
2. Control bit: 0x20
3. Token offset: 0x07
4. Token buffer: 00 0a 00 72 63 70 67 00-00 00 00 00 00 00 00 00

The dictionary is now as follows.

1. WritePosition: 226
2. 0 1 2 3 4 5 6
3. 01234567890123456789012345678901234567890123456789012345678901234
4. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
5. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
6. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
7. 0195: b\i\u\tab\tx{\rtf1\ansi\ansicpg
8. Nonprintable characters:
9. Position:0168 Byte:0x0d
10. Position:0169 Byte:0x0a

The input data is now: "1252\pard hello world}<CR><LF>".

Scanning the dictionary from index zero to index 226, new matches are located.

The first match is located at index 5. The '1' character is matched, and is moved to the dictionary write index. The largest match is now 1 character. Continuing scanning, '1' also matches at 211, but the match length is still 1 character. Because the match length is less than 2, a literal is written to the output stream.

The control bit location in the **CONTROL** field is set to zero and the control bit is advanced.

The run information is now as follows.

1. Control byte: 0x03
2. Control bit: 0x40
3. Token offset: 0x08
4. Token buffer: 00 0a 00 72 63 70 67 31-00 00 00 00 00 00 00 00

The dictionary is now as follows.

1. WritePosition: 227
2. 0 1 2 3 4 5 6
3. 01234567890123456789012345678901234567890123456789012345678901234
4. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
5. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
6. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
7. 0195: b\i\u\tab\tx{\rtf1\ansi\ansicpg1
8. Nonprintable characters:
9. Position:0168 Byte:0x0d
10. Position:0169 Byte:0x0a

The input data is now: "252\pard hello world}<CR><LF>".

Scanning the dictionary from index zero to index 227, new matches are located.

The first match is located at index 29. The '2' character is matched, and is moved to the dictionary write index. The largest match is now 1 character. Continuing scanning, '2' also matches at 192, but the match length is still 1 character. Because the match length is less than 2, a literal is written to the output stream.

The control bit location in the **CONTROL** field is set to zero and the control bit is advanced.

The run information is now as follows.

1. Control byte: 0x03
2. Control bit: 0x80
3. Token offset: 0x09
4. Token buffer: 00 0a 00 72 63 70 67 31-32 00 00 00 00 00 00 00

The dictionary is now as follows.

1. WritePosition: 228
2. 0 1 2 3 4 5 6
3. 01234567890123456789012345678901234567890123456789012345678901234
4. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
5. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
6. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
7. 0195: b\i\u\tab\tx{\rtf1\ansi\ansicpg12
8. Nonprintable characters:
9. Position:0168 Byte:0x0d
10. Position:0169 Byte:0x0a

The input data is now: "52\pard hello world}<CR><LF>".

Scanning the dictionary from index zero to index 228 for the character '5' results in zero matches.

Because the character is unmatched, it has to be moved to the dictionary write index. Because the match length is less than 2, a literal is also written to the output stream.

The control bit location in the **CONTROL** field is set to zero and the control bit is advanced.

In addition, because the control bit is now 0x80, it is not advanced; rather, the run is now written to the output.

The run information is now as follows.

1. Control byte: 0x03
2. Control bit: 0x80
3. Token offset: 0x0a
4. Token buffer: 00 0a 00 72 63 70 67 31-32 35 00 00 00 00 00 00

This is written to the output by writing the **CONTROL** field followed by token offset (0x0a) bytes from the token buffer. The output cursor is advanced by the number of bytes (0x0b) written to the output. The output is now as follows.

1. Output cursor: 0x1b
2. 000000: 00 00 00 00 00 00 00 00-4c 5a 46 75 00 00 00 00
3. 000010: 03 00 0a 00 72 63 70 67-31 32 35 00 00 00 00 00
4. 000020: 00 00 00 00 00 00 00 00-00 00 00 00 00 00 00 00
5. 000030: 00 00 00 00 00 00 00 00-00 00 00 00 00 00 00 00

This run is now complete.

#### Run 2

Prepare the next run by resetting the run information. The run information is now as follows.

1. Control byte: 0x00
2. Control bit: 0x01
3. Token offset: 0x00
4. Token buffer: 00 0a 00 72 63 70 67 31-32 00 00 00 00 00 00 00

Note that there is no need to overwrite data in the token buffer; that will be done as tokens are added.

1. Current Dictionary (WritePosition=229):
2. 0 1 2 3 4 5 6
3. 01234567890123456789012345678901234567890123456789012345678901234
4. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
5. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
6. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
7. 0195: b\i\u\tab\tx{\rtf1\ansi\ansicpg125
8. Nonprintable characters:
9. Position:0168 Byte:0x0d
10. Position:0169 Byte:0x0a

Input data is "2\pard hello world}<CR><LF>".

Add literal '2'; run information is as follows.

1. Control byte: 0x00
2. Control bit: 0x02
3. Token offset: 0x01
4. Token buffer: 32 0a 00 72 63 70 67 31-32 00 00 00 00 00 00 00

Input data is now "\pard hello world}<CR><LF>".

Add a dictionary reference (0x0af3) for the match of length 5 at offset 175 (matching "\pard"); the run information is as follows.

1. Control byte: 0x02
2. Control bit: 0x04
3. Token offset: 0x03
4. Token buffer: 32 0a f3 72 63 70 67 31-32 00 00 00 00 00 00 00

Input data is now " hello world}<CR><LF>".

Add literal ' '; the run information is as follows.

1. Control byte: 0x02
2. Control bit: 0x08
3. Token offset: 0x04
4. Token buffer: 32 0a f3 20 63 70 67 31-32 00 00 00 00 00 00 00

Input data is now "hello world}<CR><LF>".

Add a literal 'h'; the run information is as follows.

1. Control byte: 0x02
2. Control bit: 0x10
3. Token offset: 0x05
4. Token buffer: 32 0a f3 20 68 70 67 31-32 00 00 00 00 00 00 00

Input data is now "ello world}<CR><LF>".

Add a literal 'e'; the run information is as follows.

1. Control byte: 0x02
2. Control bit: 0x20
3. Token offset: 0x06
4. Token buffer: 32 0a f3 20 68 65 67 31-32 00 00 00 00 00 00 00

Input data is now "llo world}<CR><LF>".

Add literal 'l'; the run information is as follows.

1. Control byte: 0x02
2. Control bit: 0x40
3. Token offset: 0x07
4. Token buffer: 32 0a f3 20 68 65 6c 31-32 00 00 00 00 00 00 00

Input data is "lo world}<CR><LF>".

Add dictionary reference (0x0900) for a match of length 2 at offset 144 (matching "lo"); the run information is as follows.

1. Control byte: 0x42
2. Control bit: 0x80
3. Token offset: 0x09
4. Token buffer: 32 0a f3 20 68 65 6c 09-00 00 00 00 00 00 00 00

Input data is now " world}<CR><LF>".

Add literal ' '. Because the control bit is 0x80, the run is now complete. The run information is as follows.

1. Control byte: 0x42
2. Control bit: 0x80
3. Token offset: 0x0a
4. Token buffer: 32 0a f3 20 68 65 6c 09-00 20 00 00 00 00 00 00

Write the run to the output, which is now as follows.

1. Output cursor: 0x26
2. 000000: 00 00 00 00 00 00 00 00-4c 5a 46 75 00 00 00 00
3. 000010: 03 00 0a 00 72 63 70 67-31 32 35 42 32 0a f3 20
4. 000020: 68 65 6c 09 00 20 00 00-00 00 00 00 00 00 00 00
5. 000030: 00 00 00 00 00 00 00 00-00 00 00 00 00 00 00 00

#### Run 3

Prepare the next run by resetting the run information. The run information is now as follows.

1. Control byte: 0x00
2. Control bit: 0x01
3. Token offset: 0x00
4. Token buffer: 32 0a f3 20 68 65 6c 09-00 20 00 00 00 00 00 00
5. Current Dictionary (WritePosition=242):
6. 0 1 2 3 4 5 6
7. 01234567890123456789012345678901234567890123456789012345678901234
8. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
9. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
10. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
11. 0195: b\i\u\tab\tx{\rtf1\ansi\ansicpg1252\pard hello
12. Nonprintable characters:
13. Position:0168 Byte:0x0d
14. Position:0169 Byte:0x0a

Input:"world}<CR><LF>"

Add literal 'w'; run information is as follows.

1. Control byte: 0x00
2. Control bit: 0x02
3. Token offset: 0x01
4. Token buffer: 77 0a f3 20 68 65 6c 09-00 20 00 00 00 00 00 00

Input:"orld}<CR><LF>"

Add dictionary reference (0x05b0) or match of length 2 at offset 91 (matching "or"); run information is as follows.

1. Control byte: 0x02
2. Control bit: 0x04
3. Token offset: 0x03
4. Token buffer: 77 05 b0 20 68 65 6c 09-00 20 00 00 00 00 00 00

Input: "ld}<CR><LF>"

Add literal 'l'; run information is as follows.

1. Control byte: 0x02
2. Control bit: 0x08
3. Token offset: 0x04
4. Token buffer: 77 05 b0 6c 68 65 6c 09-00 20 00 00 00 00 00 00

Input: "d}<CR><LF>"

Add literal 'd'; run information is as follows.

1. Control byte: 0x02
2. Control bit: 0x10
3. Token offset: 0x05
4. Token buffer: 77 05 b0 6c 64 65 6c 09-00 20 00 00 00 00 00 00

Input: "}<CR><LF>"

Add literal '}'; run information is as follows.

1. Control byte: 0x02
2. Control bit: 0x20
3. Token offset: 0x06
4. Token buffer: 77 05 b0 6c 64 7d 6c 09-00 20 00 00 00 00 00 00

Input: "<CR><LF>"

Add dictionary reference (0x0a80) for match of length 2 at offset 168 (matching "<CR><LF>"; run information is as follows.

1. Control byte: 0x22
2. Control bit: 0x40
3. Token offset: 0x08
4. Token buffer: 77 05 b0 6c 64 7d 0a 80-00 20 00 00 00 00 00 00

Input: <EMPTY>

Add a dictionary reference for termination. Because the dictionary's write cursor is 250, the reference is 0x0fa0. Run information is as follows.

1. Control byte: 0x62
2. Control bit: 0x80
3. Token offset: 0x0a
4. Token buffer: 77 05 b0 6c 64 7d 0a 80-0f a0 00 00 00 00 00 00

The run is now complete and is written to the output, as follows.

1. Output cursor: 0x31
2. 000000: 00 00 00 00 00 00 00 00-4c 5a 46 75 00 00 00 00
3. 000010: 03 00 0a 00 72 63 70 67-31 32 35 42 32 0a f3 20
4. 000020: 68 65 6c 09 00 20 62 77-05 b0 6c 64 7d 0a 80 0f
5. 000030: a0 00 00 00 00 00 00 00-00 00 00 00 00 00 00 00

Having read through the input and written to the output, the header can now be filled in with the following:

RAWSIZE: 43

COMPSIZE: 45

CRC: 0xa7c7c5f1 (generated from bytes 0x0010 through 0x0030)

This results in the final output, as follows.

1. Output cursor: 0x31
2. 000000: 2d 00 00 00 2b 00 00 00-4c 5a 46 75 f1 c5 c7 a7
3. 000010: 03 00 0a 00 72 63 70 67-31 32 35 42 32 0a f3 20
4. 000020: 68 65 6c 09 00 20 62 77-05 b0 6c 64 7d 0a 80 0f
5. 000030: a0 00 00 00 00 00 00 00-00 00 00 00 00 00 00 00

The output is 0x031 bytes long.

### Example 2: Compressing with Tokens that Cross WritePosition

This example compresses the following [**RTF**](#gt_a9aa8673-7798-4eba-a048-8b7c95a7b080) data.

"{\rtf1 WXYZWXYZWXYZWXYZWXYZ}"

#### Initialization

The dictionary is initialized with the data, as described in section [2.3.2.1](#Section_de37d28fe4a84bbb9121704fb5d6e257). After the initialization, the dictionary is as follows.

1. WritePosition: 207
2. 0 1 2 3 4 5 6
3. 01234567890123456789012345678901234567890123456789012345678901234
4. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
5. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
6. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
7. 0195: b\i\u\tab\tx
8. Nonprintable characters:
9. Position:0168 Byte:0x0d
10. Position:0169 Byte:0x0a

CRC: 0 (zero)

COMPSIZE: 0x000C

COMPTYPE: 0x75465a4c

Output is as follows.

1. Output cursor: 0x10
2. 000000: 00 00 00 00 00 00 00 00-4c 5a 46 75 00 00 00 00
3. 000010: 00 00 00 00 00 00 00 00-00 00 00 00 00 00 00 00
4. 000020: 00 00 00 00 00 00 00 00-00 00 00 00 00 00 00 00
5. 000030: 00 00 00 00 00 00 00 00-00 00 00 00 00 00 00 00

InputCursor is: 0 (zero)

#### Run 1

Start by initializing the run information, as follows.

1. Control byte: 0x00
2. Control bit: 0x01
3. Token offset: 0x00
4. Token buffer: 00 00 00 00 00 00 00 00-00 00 00 00 00 00 00 00

Input data is "{\rtf1 WXYZWXYZWXYZWXYZWXYZ}".

Add a dictionary reference (0x0004) for a match of length 6 at offset zero (matching "{\rtf1"); run information is as follows.

1. Control byte: 0x01
2. Control bit: 0x02
3. Token offset: 0x02
4. Token buffer: 00 04 00 00 00 00 00 00-00 00 00 00 00 00 00 00

Input data is now "WXYZWXYZWXYZWXYZWXYZ}".

Add literals ' ', 'W', 'X', 'Y', 'Z'; run information is as follows.

1. Control byte: 0x01
2. Control bit: 0x40
3. Token offset: 0x07
4. Token buffer: 00 04 20 57 58 59 5a 00-00 00 00 00 00 00 00 00

Input data is now "WXYZWXYZWXYZWXYZ}".

The dictionary is now as follows.

1. WritePosition: 218
2. 0 1 2 3 4 5 6
3. 01234567890123456789012345678901234567890123456789012345678901234
4. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
5. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
6. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
7. 0195: b\i\u\tab\tx{\rtf1 WXYZ
8. Nonprintable characters:
9. Position:0168 Byte:0x0d
10. Position:0169 Byte:0x0a

A match is found for the "WXYZ" at offset 214 in the dictionary, but because each character is added to the dictionary as it is matched, following the match of the initial 4 characters of the input, the dictionary is as follows.

1. WritePosition: 222
2. 0 1 2 3 4 5 6
3. 01234567890123456789012345678901234567890123456789012345678901234
4. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
5. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
6. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
7. 0195: b\i\u\tab\tx{\rtf1 WXYZWXYZ
8. Nonprintable characters:
9. Position:0168 Byte:0x0d
10. Position:0169 Byte:0x0a

The match cursor of the input is now pointing at a 'W', as is the match cursor (at offset 218) of the dictionary. Therefore, matching continues, adding characters to the dictionary that can be matched later in the match. This terminates when a match of length 16 is found at offset 214 and the dictionary is as follows.

1. WritePosition: 234
2. 0 1 2 3 4 5 6
3. 01234567890123456789012345678901234567890123456789012345678901234
4. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
5. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
6. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
7. 0195: b\i\u\tab\tx{\rtf1 WXYZWXYZWXYZWXYZWXYZ
8. Nonprintable characters:
9. Position:0168 Byte:0x0d
10. Position:0169 Byte:0x0a

As a result, a dictionary reference (0x0d6e) is added for a length of 16 at offset 214 (matching " WXYZWXYZWXYZWXYZWXYZ"); run information is as follows.

1. Control byte: 0x41
2. Control bit: 0x80
3. Token offset: 0x09
4. Token buffer: 00 04 20 57 58 59 5a 0d-6e 00 00 00 00 00 00 00

Input data is now "}".

Add literal '}'; run information is as follows.

1. Control byte: 0x41
2. Control bit: 0x80
3. Token offset: 0x0a
4. Token buffer: 00 04 20 57 58 59 5a 0d-6e 7d 00 00 00 00 00 00

Because the control bit was 0x80, the run is written to the output, as follows.

1. Output cursor: 0x1b
2. 000000: 00 00 00 00 00 00 00 00-4c 5a 46 75 00 00 00 00
3. 000010: 41 00 04 20 57 58 59 5a-0d 6e 7d 00 00 00 00 00
4. 000020: 00 00 00 00 00 00 00 00-00 00 00 00 00 00 00 00
5. 000030: 00 00 00 00 00 00 00 00-00 00 00 00 00 00 00 00

#### Run 2

Start by initializing the run information, as follows.

1. Control byte: 0x00
2. Control bit: 0x01
3. Token offset: 0x00
4. Token buffer: 00 04 20 57 58 59 5a 0d-6e 7d 00 00 00 00 00 00

The dictionary is as follows.

1. WritePosition: 235
2. 0 1 2 3 4 5 6
3. 01234567890123456789012345678901234567890123456789012345678901234
4. 0000: {\rtf1\ansi\mac\deff0\deftab720{\fonttbl;}{\f0\fnil \froman \fswi
5. 0065: ss \fmodern \fscript \fdecor MS Sans SerifSymbolArialTimes New Ro
6. 0130: manCourier{\colortbl\red0\green0\blue0\_\_\par \pard\plain\f0\fs20\
7. 0195: b\i\u\tab\tx{\rtf1 WXYZWXYZWXYZWXYZWXYZ}
8. Nonprintable characters:
9. Position:0168 Byte:0x0d
10. Position:0169 Byte:0x0a

Input data is <EMPTY>.

Because the input data is empty, a dictionary reference (0x0eb0) of length zero is added for the WritePosition; the run is as follows.

1. Control byte: 0x01
2. Control bit: 0x02
3. Token offset: 0x02
4. Token buffer: 0e b0 20 57 58 59 5a 0d-6e 7d 00 00 00 00 00 00

This is written to the output, as follows.

1. Output cursor: 0x1e
2. 000000: 00 00 00 00 00 00 00 00-4c 5a 46 75 00 00 00 00
3. 000010: 41 00 04 20 57 58 59 5a-0d 6e 7d 01 0e b0 00 00
4. 000020: 00 00 00 00 00 00 00 00-00 00 00 00 00 00 00 00
5. 000030: 00 00 00 00 00 00 00 00-00 00 00 00 00 00 00 00

Finish by writing the header information:

RAWSIZE: 0x1a

COMPSIZE: 0x1c

CRC: 0x514bd4e2 (generated from bytes 0x0010 through 0x001d)

This results in the final output, as follows.

1. Output cursor: 0x1e
2. 000000: 1a 00 00 00 1c 00 00 00-4c 5a 46 75 e2 d4 4b 51
3. 000010: 41 00 04 20 57 58 59 5a-0d 6e 7d 01 0e b0 00 00
4. 000020: 00 00 00 00 00 00 00 00-00 00 00 00 00 00 00 00
5. 000030: 00 00 00 00 00 00 00 00-00 00 00 00 00 00 00 00

The output is 0x1e bytes long.

## Generating the CRC

### Example of CRC Generation

This example computes the value of the **CRC** field, as described in section [2.1.3.1.1](#Section_a1f226ed31e345659d26af3c6714c93f), of the following bytes (the compressed input from section [3.1.1](#Section_029bff748c00402eac2b0210a5f57371), with the header removed).

1. 03 00 0a 00 72 63 70 67-31 32 35 42 32 0a f3 20
2. 68 65 6c 09 00 20 62 77-05 b0 6c 64 7d 0a 80 0f
3. a0

The computation uses the procedure described in section [2.1.3.2](#Section_a395d09082f64ac085c4057678b2c8e8).

#### Initialization

The **CRC** field, as described in section [2.1.3.1.1](#Section_a1f226ed31e345659d26af3c6714c93f), is initially set to 0x00000000. The values in **crcTableValue** are also initialized, as described in section [2.1.2.2.1](#Section_2500f63ea1ec4605a80dd41ab63e80e9).

#### First Byte

The first byte is 0x03, and the current value of the **CRC** field, as described in section [2.1.3.1.1](#Section_a1f226ed31e345659d26af3c6714c93f), is 0x00000000, so the **tablePosition** field is computed as follows.

1. tablePosition= (0x00000000 XOR 0x03) BITWISE-AND 0xff
2. = 0x00000003

This is used to index into the **crcTableValue** field, getting a table value of the following.

1. tableValue= 0x990951ba

The **intermediateValue** field is computed as follows.

1. intermediateValue= 0x00000000 RIGHTSHIFTED by 8 bits
2. = 0x00000000

The **CRC** field that incorporates this initial byte is now as follows.

1. CRC= 0x990951ba XOR 0x00000000
2. = 0x990951ba

#### Second Byte

The next byte is 0x00, and the current value for the **CRC** field, as described in section [2.1.3.1.1](#Section_a1f226ed31e345659d26af3c6714c93f), is 0x990951ba, so the **tablePosition** field is computed as follows.

1. tablePosition= (0x990951ba XOR 0x00) BITWISE-AND 0xff
2. = 0xba

From which the **tableValue** field is as follows.

1. tableValue= 0x2bb45a92

The **intermediateValue** field is now as follows.

1. intermediateValue= 0x990951ba RIGHTSHIFTED by 8 bits
2. = 0x00990951

The updated **CRC** field is as follows.

1. CRC= 0x2bb45a92 XOR 0x00990951
2. = 0x2b2d53c3

#### Continuation

The computation proceeds as described, incorporating each byte into the value of the **CRC** field, as described in section [2.1.3.1.1](#Section_a1f226ed31e345659d26af3c6714c93f).

The final value of the **CRC** field of this set of input bytes is 0xA7C7C5F1.

# Security

## Security Considerations for Implementers

Because the compressed content could originate from a malicious source, an implementer needs to be aware that certain sizes, such as COMPSIZE and RAWSIZE, might have been tampered with. Care needs to be taken to ensure that the client does not attempt to read or access data that is larger than the input during decompression. Few security risks exist during compression, as the algorithm can compress any content (not just [**RTF**](#gt_a9aa8673-7798-4eba-a048-8b7c95a7b080)), and operates on the byte level.

## Index of Security Parameters

None.

# Appendix A: Product Behavior

The information in this specification is applicable to the following Microsoft products or supplemental software. References to product versions include updates to those products.

* Microsoft Exchange Server 2003
* Microsoft Exchange Server 2007
* Microsoft Exchange Server 2010
* Microsoft Exchange Server 2013
* Microsoft Exchange Server 2016
* Microsoft Office Outlook 2003
* Microsoft Office Outlook 2007
* Microsoft Outlook 2010
* Microsoft Outlook 2013
* Microsoft Outlook 2016
* Microsoft Exchange Server 2019
* Microsoft Outlook 2019
* Microsoft Outlook 2021

Exceptions, if any, are noted in this section. If an update version, service pack or Knowledge Base (KB) number appears with a product name, the behavior changed in that update. The new behavior also applies to subsequent updates unless otherwise specified. If a product edition appears with the product version, behavior is different in that product edition.

Unless otherwise specified, any statement of optional behavior in this specification that is prescribed using the terms "SHOULD" or "SHOULD NOT" implies product behavior in accordance with the SHOULD or SHOULD NOT prescription. Unless otherwise specified, the term "MAY" implies that the product does not follow the prescription.

# Change Tracking

This section identifies changes that were made to this document since the last release. Changes are classified as Major, Minor, or None.

The revision class **Major** means that the technical content in the document was significantly revised. Major changes affect protocol interoperability or implementation. Examples of major changes are:

* A document revision that incorporates changes to interoperability requirements.
* A document revision that captures changes to protocol functionality.

The revision class **Minor** means that the meaning of the technical content was clarified. Minor changes do not affect protocol interoperability or implementation. Examples of minor changes are updates to clarify ambiguity at the sentence, paragraph, or table level.

The revision class **None** means that no new technical changes were introduced. Minor editorial and formatting changes may have been made, but the relevant technical content is identical to the last released version.

The changes made to this document are listed in the following table. For more information, please contact dochelp@microsoft.com.

| Section | Description | Revision class |
| --- | --- | --- |
| [5](#Section_38d1252a0b714dc3bce43afa752d200e) Appendix A: Product Behavior | Updated list of supported products. | major |

# Index

A

Abstract data model

 [common](#section_d7604c1e98f04b8bb91f051d3db228e1) 9

 [compression](#section_4209102164ad49e9a5a7b3ba6ab87a69) 15

 [decompression](#section_7cbd5bef2e25426684a9d25ebcba3d5a) 13

[Applicability](#section_2f4645cae37a436ca8adde9256a6abf9) 8

C

[Change tracking](#section_02b7024710fc4a3694808609cba8ad7e) 45

Common

 [abstract data model](#section_d7604c1e98f04b8bb91f051d3db228e1) 9

[Compressing with tokens that cross WritePosition example](#section_59eb3a356ee14a0893b9b9f4a7e3a0ca) 37

Compression

 [abstract data model](#section_4209102164ad49e9a5a7b3ba6ab87a69) 15

[CRC generation example](#section_9c6fbcd5cc30480eb1f1a84edc79db97) 41

D

Data model – abstract

 [common](#section_d7604c1e98f04b8bb91f051d3db228e1) 9

 [compression](#section_4209102164ad49e9a5a7b3ba6ab87a69) 15

 [decompression](#section_7cbd5bef2e25426684a9d25ebcba3d5a) 13

[Decompressing Compressed RTF example](#section_bf6f7e5149394e169b446bd644e9ae5d) 20

Decompression

 [abstract data model](#section_7cbd5bef2e25426684a9d25ebcba3d5a) 13

E

Examples

 [compressing with tokens that cross WritePosition](#section_59eb3a356ee14a0893b9b9f4a7e3a0ca) 37

 [CRC generation](#section_9c6fbcd5cc30480eb1f1a84edc79db97) 41

 [Decompressing Compressed RTF](#section_bf6f7e5149394e169b446bd644e9ae5d) 20

 [reading a token from the dictionary that crosses WritePosition](#section_421a2da57752498589810f19f1e5b687) 25

 [simple RTF](#section_ba662823d47a4db3ad45a368a82acc90) 28

G

[Glossary](#section_46f34c09a8f44b09b4286ece309e0bc5) 7

I

[Implementer - security considerations](#section_6f1c39553dbd4c90b95bdcbb3791fb54) 43

[Index of security parameters](#section_517e55c4d7a648308a23b98b527eef94) 43

[Informative references](#section_85c0b884a9604d1a874e53eeee527ca6) 8

[Introduction](#section_401931f6fca34644ab5f41df4b1c22c6) 7

N

[Normative references](#section_3974dad6f55944f1954258d7823094ab) 8

O

[Overview (synopsis)](#section_3f4a925eece549858a9e13719ab08302) 8

P

[Parameters - security index](#section_517e55c4d7a648308a23b98b527eef94) 43

[Product behavior](#section_38d1252a0b714dc3bce43afa752d200e) 44

R

[Reading a token from the dictionary that crosses WritePosition example](#section_421a2da57752498589810f19f1e5b687) 25

References

 [informative](#section_85c0b884a9604d1a874e53eeee527ca6) 8

 [normative](#section_3974dad6f55944f1954258d7823094ab) 8

S

Security

 [implementer considerations](#section_6f1c39553dbd4c90b95bdcbb3791fb54) 43

 [parameter index](#section_517e55c4d7a648308a23b98b527eef94) 43

[Simple RTF example](#section_ba662823d47a4db3ad45a368a82acc90) 28

[Standards assignments](#section_230766aa89af493db6d7d45e68f17e5d) 8

T

[Tracking changes](#section_02b7024710fc4a3694808609cba8ad7e) 45